**UV CURABLE**

**坤隆新材料**

|  |
| --- |
| **HM-107****Product description：** HM-107 is an amine modified acrylate with light color, low odor,non-reddening.**Qualification：**Project Target Test Method |
| Appearance | Transparent viscous liquid | Visualization |
| Chromaticity（APHA） | ≤1 | GB/T 3143-1982(platinum-cobalt method) |
| Functionality |  2 | Theoretical Value |
| Viscosity（mpa.s/25℃) | 80 | GB/T 2794-1995 |

**Application field：**Coating, Ink.

 **Matters need attention:**

Store this product in a cool,dry place where the ambient,temperature is below 40degrees Celsius. The shelf is 180 days. This product has no spontaneous combustion and explosive, low corrosion, wear gloves and masks, avoid skin contact and inhalation as far as possible. If the skin adheres to the skin, wipe it with alcohol and then rinse it with water. If invading the eye, you should immediately rinse with a large amount of normal saline, and please seek medical attention if necessary.

**Packaging specification：** 25Kg， 200Kg

Company name：Jiangxi Kunong New Material Co,LTD

Address：Ecological Industrial Park, Tonggu County, Jiangxi Province

Contact person： Miss Zou 13707490831

Mr.Zou 18170533822

Technical service：Mr.Hou 18670782966